Permit # \_\_\_\_\_\_\_

Authorized by:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

County of Bruce

#  Transportation & Environmental Services Department

 Box 398, 30 Park Street, Walkerton, Ontario N0G 2V0 (519) 881-2400 Fax: (519) 507-3030 TransportationInfo@brucecounty.on.ca

**Single/Annual Trip Permit – M2**

***For Vehicles and Loads between 3.76m and 4.99m in total width, up to 45.75m long or between 63,500 kg & 120,000 kg***

*Pursuant to HTA RSO 1990 Chapter H. 8 Part VII, Section 110.1 and Current Bruce County By-Law to Prohibit Activity*

Name of Applicant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Town/City: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Province: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Postal Code: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Telephone: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Fax: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Email Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Description of Vehicle and Load: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Dimensions and Weight of Load:

Width: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(m) Length:\_\_\_\_\_\_\_\_\_\_\_\_(m) Height: \_\_\_\_\_\_\_\_\_\_\_\_\_\_(m) Weight: \_\_\_\_\_\_\_\_\_\_\_\_ (kg)

Total # of Axles including Steering Axles: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

SUBMIT details and sketch of axle spacing, tire sizes and axle loads with application.

❑ **Single Trip**: **$65**

**Valid \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ to \_\_\_\_\_\_\_\_\_\_\_\_\_\_**

*(A three-day grace period is permitted)*

Exact route to be followed:

­­­­­­­­­­­­­­­­­

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**❑ Annual Permit**: **$250**

**Valid January 1, 20\_\_\_ to December 31, 20\_\_\_**

This permit covers all roads under the jurisdiction of the Bruce County Transportation and Environmental Services.

\*Gross Vehicle and Load Weight must not exceed 63,500 kgs. When load exceeds 63,500 kgs, it is considered a single trip

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_­­­­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Liability Insurance ($2,000,000.00 minimum): Name of Insurance Company: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Policy No.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Amount: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Expiry Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The Owner/Mover of the load being moved shall indemnify and save harmless the County of Bruce against any actions, claims, damages, loss, or other proceedings, by whomever brought or made based upon, occasioned by or attributed to the issuance of the permit.

I hereby certify that the information on this application is a true statement.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date of Application Name of Applicant or Agent

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Signature of Applicant or Agent

**SPECIFIC CONDITIONS:**

a) No moving can take place without an authorized permit. Permit is non-transferable.

b) Details and sketch of axle spacing, tire sizes and axle loads must be submitted with application.

c) This Permit must be carried in the vehicle and produced on demand of a Police Officer or an Officer appointed for

 carrying out the provisions of the Highway Traffic Act.

d) It is the mover's responsibility to ensure the route selected is suitable, which includes notifying any utility companies.

 e) Where heights exceed 4.15 metres, approval is required from utility companies. See Appendix A on the Bruce County website.

f) Move must take place during daylight hours, half hour after sunrise to half hour before sunset. Moves are not permitted on Saturdays, Sundays and Statutory Holidays, and in congested areas between the hours of

 7:00 a.m. to 9:30 a.m. or between the hours of 4:00 p.m. to 6:30 p.m.

g) Moves must not be carried out in periods of limited visibility or upon any accumulation of snow on the roadway

 or if the continuous use of windshield wipers is required.

 h) Vehicles and/or loads in excess of dimensions prescribed under Section 109 of the Highway Traffic Act shall be marked with bright red or orange warning flags of not less than 40 cm. square and shall be mounted to the extremities of the vehicle or load. The flag(s) must be kept in good and clean condition so as not to diminish their effectiveness.

i) Weight restrictions/load posting on several roads throughout the Bruce County Transportation & Environmental

 Services Department’s jurisdiction must be adhered to during spring thaw conditions. Refer to the Bruce County Website for a map of weight restrictions/load posted roads.

# j) Farm Vehicle Exemption - Over-dimensional farm vehicles are exempt from permit requirements when the vehicle is self-propelled or drawn by a farm tractor.

k) The Permit holder assumes all responsibility for damages that may be caused to the highway due to driving, operating

 or moving of any such heavy vehicle, load, object or structures. (HTA RSO 1990 c. H8 s. 110(5). This includes public

 utility overhead wires, structures, or encroachments.

l) Convoy moves are not permitted. Each load must be separated by at least 45 minutes. When on route, a minimum spacing of 10km is required.

m) **Allow 5 business days for the permit to be issued by the Transportation & Environmental Services Department.**

 **ESCORT REQUIREMENTS:**

**A PRIVATE ESCORT WARNING VEHICLE IS REQUIRED WHEN VEHICLE AND LOAD IS:**

**LENGTH:** From 36.76 m to 45.74 m - one escort vehicle required at rear.

Overhang greater than 4.65 m - one escort vehicle required on the rear of load.

**HEIGHT:** 4.87 m and greater - one escort vehicle (pole car) required.

**WIDTH:** From 4 m to 4.59 m – one escort vehicle

From 4.6 m to 4.99 m – two escort vehicles